**Buccaneer Website Content**

HOME

ABOUT (overview)

Coating Systems

APPLICATIONS (overview)

Walls

Roofing

Wood

Floors & Driveways

Decks & Balconies

Cracks

CONTACT

Request Info form

LEGAL/PRIVACY POLICY

**HOME (**[**www.buccaneerprotectivecoatings.com**](http://www.buccaneerprotectivecoatings.com)**)**

*Content to come based on finalized content of internal pages.*

Carousal (rotating images):

**SLIDE 1**

**Title:** Architectural and Industrial Coating Systems

**Description:** Aunique chemical formula creating maximum durability that outperforms conventional paint products, and gives any building or structure a superior life span.

**Link:** Links to (www.buccaneerprotectivecoatings.com/coatingsystems)

**SLIDE 2**

**Title:** Applications

**Description:** High quality protective coatings specific to the requirements of several distinct applications, from walls to driveways.

**Link:** ([www.buccaneerprotectivecoatings.com/applications](http://www.buccaneerprotectivecoatings.com/applications))

**SLIDE 3**

**Title:** S-26 Plastic Wall Coating System

**Description:** This featured product offers leak and moisture protection for outdoor walls, providing resistance to extreme temperature changes and ultraviolet light exposure.

**Link:** ([www.buccaneerprotectivecoatings.com/walls](http://www.buccaneerprotectivecoatings.com/walls))

**About**

Buccaneer Canada is a manufacturer and distributor of Architectural and Industrial Coating Systems designed to preserve and protect a wide spectrum of building materials and surfaces.

**Walls**

Resistance to extreme temperature changes and ultraviolet light exposure.

**Roofing**

Cold process roofing system suitable for a wide cross-section of roofing substrates.

**Wood**

Flexible and durable products capable of expanding and contracting to prevent cracking.

**Floors & Driveways**

Preventing damage caused by moisture. Protection against alkalis, ultraviolet light and staining.

**Decks & Balconies**

Seamless floor casing resistant to UV damage, temperature fluctuations and chemicals.

**Cracks**

Flexible and waterproof. Designed to move with a structure’s substrata to prevent cracking.

**ABOUT** (overview) ([www.buccaneerprotectivecoatings.com/about](http://www.buccaneerprotectivecoatings.com/about))

Based in Calgary, Alberta, Buccaneer Canada *(link to internal page on company)* is a manufacturer and distributor of Architectural and Industrial Coating Systems *(link to internal page on Industrial systems)* designed to preserve and protect a wide spectrum of building materials and surfaces. Learn more about our applications.

Buccaneer coating solutions have a 35-year history of development and application in the United Kingdom and South Africa. Over the years applications have spread throughout South Africa, the Benelux Countries, Iceland, and Canada.

At Buccaneer, our mission is to produce the highest quality coatings utilizing our proprietary formulations with uncompromising raw material inputs. Combining ease of use and superior durability provides a cost effective and long term coating solution for our customers while respecting the environment by using only eco-friendly acceptable raw materials that are not hazardous to people, animals or the environment.

**COATING SYSTEMS** (www.buccaneerprotectivecoatings.com/coatingsystems)

**Architectural and Industrial Coating Systems**

One of the first questions we typically get at Buccaneer is “why plastic, why not paint?”. Our plastic architectural and industrial coating systems have proved themselves as far more durable than conventional paints and varnishes.

Plastics do not degrade over time or become a hazard. Instead, they protect and preserve the surfaces *(link to applications)* to which they are applied.

Extensive research and development has led to the advancement of proprietary resins and entirely unique formulations. Buccaneer Architectural and Industrial Coating Systems can be applied to all types of surfaces *(link to applications)* including steel, wood, concrete and plaster. The unique chemical formula of this product line allows for maximum durability that will outperform virtually all conventional paint products and give any building or structure a far superior life span dramatically reducing expensive maintenance costs.

Buccaneer offers both water-borne and solvent-borne protective coating solutions based on the application required.

**APPLICATIONS** (overview) ([www.buccaneerprotectivecoatings.com/applications](http://www.buccaneerprotectivecoatings.com/applications))

Given Buccaneer's unique approach, we are able to offer high quality protective coatings specific to the requirements of several distinct applications.

**Walls** *(image required to represent)*

* Buccaneer offers total wall protection
* Leak and Moisture protection for outdoor walls such as: masonry block, concrete, plaster, stucco
* Waterproof film resistant to ultraviolet radiation and temperature fluctuations

Learn more

**Roofing** *(image required to represent)*

* Cold process roofing system
* Suitable for wide cross-section of roofing substrates - from flat to fully pitched roofs
* Ideal for steel, concrete, tile and wood surfaces

Learn more

**Wood** *(image required to represent)*

* Protection against UV exposure, water ingress, moisture and general age degradation
* Unique blend of water-soluble plastic polymers
* Durable when applied to wood siding, decks or railings
* Simple application process

Learn more

**Floors & Driveways** *(image required to represent)*

* Durable non-yellowing protective film for brick, stonework, terrazzo and concrete
* Prevention of damage caused by moisture accumulation, freeze/thaw cycles, UV exposure and general wear and tear
* Resistant to alkalis, ultraviolet light and staining
* Protection against wear and tear

Learn more

**Decks & Balconies** *(image required to represent)*

* Long-lasting coating system for concrete decks and balconies
* Solvent-borne, waterproof floor coating
* Well suited to high-traffic areas such as balconies, garage floors, driveways and parkades

Learn more

**Cracks** *(image required to represent)*

* Can be used for cement, concrete, plasterwork and woodwork
* Water soluble
* Environmentally friendly

Learn more

**WALLS** ([www.buccaneerprotectivecoatings.com/walls](http://www.buccaneerprotectivecoatings.com/walls))

The **S-26 Plastic Wall Coating System** is based on an uncompromising blend of proprietary resins; it offers the best possible leak and moisture protection for outdoor walls. This system contains a highly durable, pure acrylic binder. Once applied it provides a high strength, waterproof film with excellent elastic properties, resistance to ultraviolet radiation, as well as wide temperature fluctuations.

**The System Components - 1,2,3:**

**S-26 Stabilizing Primer**

This product is a basecoat for use on new or ageing building substrates or over existing chalky or friable paint surfaces. This primer is uniquely formulated for optimal penetration and allows for enhanced adhesion of subsequent coats. The S-26 Stabilizing Primer dries clear, and can be pigmented to augment concealing properties.

**S-26 Storm Seal HD**

This product is a highly elastic and uniquely durable waterproofing formula that will bridge hairline cracks and surface imperfections. It is able to withstand extreme temperature changes and ultraviolet light exposure.

**S-26 Wall Seal**

This product is a flexible, yet hard surface, acyclic topcoat designed to preserve and protect walls. It is ideal for a long-term decorative finish, capable of withstanding the elements.

The S-26 Wall Protection System is a 6-in-1 solution for all external wall maintenance issues:

1. All Weather Resistant;
2. Fully waterproof capable of bridging cracks, joints and surface imperfections, preventing the ingress of water and moisture into any structure;
3. Thermo plastic and will flex with any surface to without cracking due to structural movement as well as thermal expansion and contraction;
4. Preserves against general degradation;
5. Reduces maintenance costs; and
6. Decorates and upgrades any building structure.

**S-26 Concrete and Masonry**

This product is a solvent-based, fully waterproof floor coating well suited to high-traffic areas such as balconies, walls (link to walls), garage floors, and parkades. Once applied, it creates a seamless floor casing resistant to UV damage, freeze/thaw conditions and a variety of chemicals and lubricants.

Back to applications

**ROOFING** ([www.buccaneerprotectivecoatings.com/roofing](http://www.buccaneerprotectivecoatings.com/roofing))

Buccaneer offers a cold process roofing system suitable for a wide cross-section of roofing substrates from flat to fully pitched roofs.

**Sloped Roofing**

**S-26 Storm Seal LD**

This liquid plastic is a distinctive cold process roofing product that is able to stretch and flex with a wide cross-section of sloped roof substrates through extreme temperature changes. This product’s lightfast pigments will retain colour and protect its substrate against the harshest of elements including: ultraviolet light, snow, rain, and chemical pollution. It can be applied to any existing tile, metal, wood, metal, fiberglass, or asbestos roof.

**Flat Roofing**

**S-26 Storm Seal HD**

This product is an integral component of Buccaneer’s cold process roofing system. It works by forming a thick plastic skin that will remain flexible and durable while waterproofing virtually any roofing substrate including: concrete, concrete tiles, steel, wood, and asbestos.

While developing S-26 Storm Seal HD, Buccaneer focused on the foundation of the product - a Waterproof material capable of adhering to a wide cross section of substrate, with sufficient strength to bridge hairline cracks and flexibility to accommodate expansion and contraction.

Our proprietary resin and high quality pigments work to preserve this unique blend of characteristics over extended periods of exposure to the harshest ultraviolet light, environmental conditions.

**S-26 Storm Seal VHD**

A derivative of S-26 Storm Seal HD, this product incorporates plastic fibers into the mastic thereby increasing its tensile strength. Well suited for seams, joints, and transition areas were high stress torsional forces may concentrate.

**Base Coats**

Where required, Buccaneer draws on a selection of base coats to suite a full spectrum of roofing substrates.

**Polyester Fabrics**

Utilized in particularly demanding applications where extra waterproofing measures are warranted. Such surfaces include steel roof seams, joints and roof/wall transitions. Our cold seal roofing process can incorporate the use of polyester fabrics between consecutive coats of Storm Seal.

*This product is 100% environmentally friendly, is water soluble, and contains ultra-low levels of V.O.C.’s.*

Back to applications

**Wood** ([www.buccaneerprotectivecoatings.com/decks](http://www.buccaneerprotectivecoatings.com/decks))

Wood is a unique surface because it is a natural material that expands, contracts, absorbs water, and warps long after it has been hewn from a tree. Wood products are vulnerable to sunlight, insect infestation, moisture and general age degradation. Therefore, it is important for any wood preservation product to not only protect against this damage but also be able to move and flex continuously with the wood. Buccaneer’s range of wood preservation products are a unique blend of water-soluble plastic polymers that are durable and have a simple application process. They can be used on new or existing wooden structures.

**S-26 Plastic Wood Preservative**

This water borne, ultra-low VOC product is unlike any other available wood coating. It is designed for all vertical external woodwork including: garage doors, fencing, window frames, and timber homes. S-26 Plastic Wood Preservative works by forming a water resistant, mould and mildew proof barrier that is resistant to ultraviolet degradation. Once this product is applied, it maintains a flexible surface capable of expanding and contracting with the wood in order to prevent cracking during extreme temperature changes.

**S-26 Wooden Deck Coating**

This product is a derivative of the S-26 Plastic Wood Preservative. S-26 Wooden Deck Coating is a non-slip formula that ensures secure footing even in damp conditions. It was specially formulated to withstand the added rigors of foot traffic and ultra-high ultraviolet exposure.

**S-26 Clear Seal-Wood**

S-26 Clear Seal -Wood is a solvent borne, fully waterproof, clear topcoat utilized to complement S-26 Plastic Wood Preservative in high impact applications such as: outdoor furniture, railings, stair treds and decks. This product is an easy to use, single pack, quick drying formula.

Back to applications

**FLOORS & DRIVEWAYS** (www.buccaneerprotectivecoatings.com/floors)

From face brick to driveways, the S-26 flooring series prevents damage caused by moisture and is resistant to alkalis, ultraviolet light and staining. Each product in this series offers protection against the elements.

**Face Brick, Stone and Floor Sealers**

**S-26 Clear Seal - Concrete and Masonry**

This solvent based product is a penetrating sealant that provides a highly durable, non-yellowing protective film for brick, stonework, terrazzo concrete and existing epoxy finishes. It prevents damage typically caused by moisture and UV degradation and wear and tear by bonding to the surface and creating a hard wearing, waterproof barrier. S-26 Clear Seal is resistant to alkalis, ultraviolet light and staining. This is one of the most versatile, long-lasting clear plastic coatings ever developed.

**S-26 Plastic Floor Coating**

This solvent based, single pack, pigmented, plastic floor enamel protects concrete floors, balconies and exterior walkways against wear and tear caused by moisture ingress, ultraviolet radiation and extreme weather conditions. It is extremely tough, hardwearing and waterproof.

*This product is offered in a variety of colours and comes in a non-slip version.*

**S-26 Epoxy Floor Enamel**

This twin pack, pigmented, plastic floor enamel is ideal for high traffic areas prone to exposure to solvents, lubricants and other potentially corrosive fluids. It is a heavy-duty seamless floor cladding that is resistant to many harsh solvents and chemicals. Apply this enamel to floors and walls in shops or processing areas to create a seamless, sealed coating between floor and wall.

**S-26 Water Based Floor Coating**

This single pack, pigmented, plastic product has a highly durable, non-slip finish ideally suited for use in areas such as stairwells, mechanical rooms, storage areas and other confined spaces where fume buildup may pose a fire or inhalation hazard. Also, Ulta-low volatile organic compound (VOC) makes for odorless application.

Back to applications

**DECKS & BALCONIES** (www.buccaneerprotectivecoatings.com/decks)

**S-26 Concrete and Masonry**

This product is a solvent-based, fully waterproof floor coating well suited to high-traffic areas such as balconies, walls (link to walls), garage floors, and parkades. Once applied, it creates a seamless floor casing resistant to UV damage, freeze/thaw conditions and a variety of chemicals and lubricants.

Back to applications

**CRACKS** (www.buccaneerprotectivecoatings.com/cracks)

**S-26 Plastic Crack Filler**

This product can be used in any type of crack or void to repair damage in minutes. This water soluble formulation is environmentally friendly. Unlike powdered crack fillers, the S-26 Plastic Crack Filler is flexible, waterproof and will move with a structure’s substrata to prevent future cracking. Where extra hardness is desired, incorporate Portland cement into the crack filler prior to application. Crack filler can be used with cement, concrete, plasterwork and woodwork, making it one of the most versatile fillers in the world.

Back to applications

**CONTACT** (www.buccaneerprotectivecoatings.com/contact)

**Main Office**

3621B 3rd Street NE

Calgary, Alberta

T2E 5V1

Canada

Phone number: +1 (403) 452 7005  
  
Email: info@buccaneerprotectivecoatings.com

**INFO REQUEST** (www.buccaneerprotectivecoatings.com/requestinfo)

\* Information required

Name\*

Company\*

Phone\*

Email\*

Information of interest\*

Email a representative  
Request product MSDS   
Request a bid proposal  
Have a representative call you back  
Product specifications

Comments

**LEGAL** (www.buccaneerprotectivecoatings.com/legal)

Please read these terms of use carefully. By using this website, you agree to these Terms of Use without modification. Buccaneer Protective Coatings Ltd. (Buccaneer). has created this website for your use and information, subject to the following terms and conditions.

GENERAL TERMS OF USE  
  
Limitations on Copying. Buccaneer grants to you a non-exclusive and non-transferable license to view and print documents and web pages located on this website for non-commercial use only. The information and content on this website is provided to you solely for the purpose of helping you understand the services available to you at Buccaneer. The documents and web pages on this website may not be reproduced, republished, retransmitted, sold, modified or exploited in any way. Any printed copies of these web pages must retain, without modification any proprietary notices.  
  
Linked Internet Sites. Buccaneer may provide links to other Internet sites as a convenience to you. The content on these linked sites does not necessarily reflect the opinion of Buccaneer and Buccaneer assumes no liability or responsibility that may arise in relation to any such site. The inclusion of any link in this website does not imply that we recommend or endorse the linked site.

Linking to our website. Unless otherwise set forth in a written agreement between you and Buccaneer, you must adhere to our linking policy as follows:

* The appearance of the link must not damage or dilute the goodwill associated with our company;
* The link must point to the URL (www.westriverprojects.com) and not to other pages within this website;
* The appearance, position and other attributes of the link may not create the false appearance that your organization or entity is sponsored by, affiliated with or associated with Buccaneer;
* When selected by a user, the link must display this website on full screen and not within a "frame" on the linking website; and
* Buccaneer reserves the right to request the removal of the link at any time in its sole discretion.

DISCLAIMER

This website has been prepared for information purposes only and may contain errors, omissions or inaccuracies. Buccaneer assumes no liability or responsibility for any such errors, omissions or inaccuracies and makes no representations about the accuracy, reliability, completeness or timeliness of the information contained on this website. Use of this website constitutes the users acknowledgement that Buccaneer and its affiliates, shareholders, directors, officers and employees are not, and will not be subject, to any liability based on the information contained on this website, errors therein or omissions therefrom, whether or not any such persons knew, or should have known of any such errors or omissions or were responsible for or participated in the inclusion or omission of information in this website.

This website is to be used at your own risk. All information contained on this website is provided without warranty or condition of any kind, either express or implied. Buccaneer expressly disclaims all warranties and conditions with regard to such information, including, but not limited to, all implied warranties and conditions of merchantability and fitness for a particular purpose and all warranties and conditions implied by statute. In no event shall Buccaneer or its affiliates, shareholders, directors, officers or employees be liable for any damages or any kind resulting from use of this website including, without limitation, any direct, indirect, punitive, incidental, special or consequential damages arising out of or in any way connected with any information obtained from this website or any use of such information.  
  
For more information on this legal page, please contact us at info@buccaneerprotectivecoatings.com.